---
name: Bug report
about: Create a bug report to track and resolve issues -- support requests will be
  deleted
title: ''
labels: ''
assignees: ''

---

Note: Issues are not for customer support, configuration or discussion. For those topics please consult with your HW vendor or the OSMU Discord at: https://osmu.bitaxe.org

**Describe the bug**
A clear and concise description of what the bug is.

**To Reproduce**
Steps to reproduce the behavior:
1. Go to '...'
2. Click on '....'
3. Scroll down to '....'
4. See error

**Expected behavior**
A clear and concise description of what you expected to happen.

**Screenshots & Photos**
If applicable, add AxeOS screenshots and/or photos of your BluAX to help explain your problem.

**Hardware (please complete the following information):**
 - BluAX HW version: [e.g. BluAX 320, BluAX 321, etc]
 - BluAX HW vendor: [Digital Shovel](https://bluax.digitalshovel.com/)
 - ESP-Miner FW version: [e.g. 3.2.1, etc]
 - Hash Frequency:
 - Voltage:
 - Pool URL, Port, User:

**Additional context**
Add any other context about the problem here.
